








**Packet Tracer Task**



**Final Comments:**

Cisco doesn’t allow to set invalid IP’s or subnet masks in the first place, so we had to put correct IP and subnet masks for each PC.

**Bonus:**

To confirm connectivity without using **ping**, use **Tracert**. If the route is displayed, PC is reachable.